

PULSE DETECTION

* After capturing video and calculating brightness of each frame :





Frequency Response Using FFT:

